

LCT ASTROLABE

|  |  |  |
| --- | --- | --- |
| Machinery and Equipment | 3 | Principal Particular |
| Main Engine | 2x Yanmar 6EY17W @590Kw |  | Port of Registry | Dampier |
| Generator Engine | 3 x Cummins N855- DM 240kW |  | Flag  | Australia |
| Emergency Generator | Cummins 68T 80kW |  | IMO NumberCall Sign | 9766970VHKL |
| Bow Thruster | 200kW Double Direction  |  | Year Build | 2015 |
| Steering Gear | Oceanic Marine Electro Hydraulic |  | LOA | 59.60m |
| Max Speed | 10 knots |  | Breadth | 15.00 m |
| Fuel Consumption | 5.5 m3/day |  | Draft | 2.8 m |
| Cranage | Electro Hydraulic 900kg SWL |  | GRT | 1136 |
| Winches | 2 x YM1F32/3 Hydraulic Windlass |  | Displacement | 1925t |

Landing Craft

|  |  |  |
| --- | --- | --- |
| Cargo Capacities |  | Discharge Rates |
| Cargo Fresh Water | 388.6m3 |  | Cargo Fuel pumps | 2x 80m3 @0.8mpa |
| Container Stack Weight | 45t per 20ft |  | Cargo Water pumps | 2x 65m3 @0.65mpa |
| Ballast Capacity | 396.4m3 |  |  |
| Cargo Fuel Oil | 645.9m3 |  |
| Outside Deck Area | 533.8m2 |  |
| Under Cover Deck Area | 73.8m2 |  |
| Deck Cargo Capacity | 10t/m2 |  |